{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Раскладка АИС500ПТ","Блок MIG","Подающий механизм","Рисунки"],"not_rendered":{"images":10,"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Раскладка АИС500ПТ","index":0,"n_rows":109,"n_cols":7,"rows_kept":109,"flags":["formulas_cached_only"]}
[]
[null,"РАСКЛАДКА СВАРОЧНЫЙ ПОЛУАВТОМАТ АИС 500ПТ"]
{"$rows_empty":45}
[null,"Поз.","Код ELITECH","Артикул","Наименование ПОЛУАВТОМАТ АИС 500ПТ","Описание (англ.)","Комплектация"]
[null,null,"0601.050000",{"$nulls":3},1]
[null,1,"0602.030100","00.3092","Ручка","Handle (L-295)",1]
[null,2,"0602.020200","00.3051","Сведодиод (зеленый)","Abnormal LED (Φ5 Yellow)",1]
[null,3,"0602.020100","00.3050","Светодиод (красный)","Power LED (Φ5 Green)",1]
[null,4,"0602.020300","00.3052","Цифровой дисплей","Current digital  meter (LX9135-2V-A)",1]
[null,5,"0602.020400","00.3053","Переключатель кулисный","2T/4T exchange switch (KCD-19)",1]
[null,6,"0602.020400","00.3053","Переключатель кулисный","Gas checking/ working gas exchange switch (KCD-19)",1]
[null,7,"0602.020500","00.3054","Потенциометр","Collect current /welding current adjustment potentiometer (RV28P-B472)",1]
[null,8,"0602.020500","00.3054","Потенциометр","Collect voltage/Arc force current adjustment potentiometer (RV28P-B472)",1]
[null,9,"0601.040100","00.3113","Потенциометр","Inductance adjustment potentiometer (RV28P-B333)",1]
[null,10,"0601.040200","00.3114","Тумблер ","MIG/MMA exchange switch (E-TEN1321)",1]
[null,11,"0601.040300","00.3115","Цифровой дисплей","Voltage digital display (LX9135-2V-V)",1]
[null,12,"0601.050100","00.3055","Разъем \"-\" (Dx50)","Negative pole output fasten connector (50-70)",1]
[null,13,"0601.050200","00.3055","Разъем \"+\" (Dx50)","Positive pole output fasten connector (50-70)",1]
[null,14,"0601.050300","00.3135","Кожух левая часть","Left side cover (MIG500-1)",1]
[null,15,"0602.020900","00.3056","Реактор","Output reactor (13T)",1]
[null,16,"0602.021000","00.3057","Абсорбер","Absorbing curtain  (AT400DK)",1]
[null,17,"0602.030500","00.3096","Колесо малое","Small wheel (LUN-85)",2]
[null,18,"0601.050400","00.3136","Подставка для баллона","Gas xylinder trolley (MIG500-2)",1]
[null,19,"0602.030400","00.3095","Колесо большое","Big wheel (LUN-200)",2]
[null,20,"0601.050500","00.3137","Ось","Axle (MIG500-3)",1]
[null,21,"0601.050600","00.3138","Фиксатор оси","Axle locker (MIG500-4)",2]
[null,22,"0602.021300","00.3060","Конденсатор","Capacitor (SFC-450VAC/50uf)",4]
[null,23,"0602.021400","00.3061","Конденсатор","Capacitor (SFC-20UF/1400V)",2]
[null,24,"0602.030900","00.3100","Дивертор","Diverter (500A/75mV)",1]
[null,25,"0601.050700","00.3139","Фильтр индуктивный","Filter inductance (MIG500-L1)",1]
[null,26,"0602.022000","00.3067","Дефлектор вентилятора","Axial fan  (200FZY6-S/220V)",1]
[null,27,"0602.021800","00.3065","Клемма заземления","Grounding nut (8*25)",1]
[null,28,"0601.050800","00.3055","Разъем \"+\" (Dx50)","Wire feeder positive side fasten connector (50-70)",1]
[null,29,"0602.021900","00.3066","Решетка вентилятора","Fan cover (FJZ-01)",1]
[null,30,"0601.050900","00.3140","Кожух правая часть","Right side cover (MIG500-6)",1]
[null,31,"0602.022500","00.3072","Диод","Fast recover diode (DH2F100N4S)",3]
[null,32,"0602.022600","00.3073","Нагрузочная катушка","Load coil (FZ-01)",1]
[null,33,"0602.021700","00.3064","Дефлектор","Wind shield (DF-01)",1]
[null,34,"0602.023200","00.3079","Конденсатор","Capacitor (SFC-500VAC/4.0uf)",1]
[null,35,"0601.051000","00.3141","Катушка индуктивная","Saturated inductance (MIG500-L3)",1]
[null,36,"0602.023300","00.3080","Датчик Холла","Current feedback board (AT400NBH)",1]
[null,37,"0602.021600","00.3063","Выпрямитель","3phs rectifier (MDS100/16E)",1]
[null,38,"0602.022900","00.3076","Термовыключатель","Thermal switch (MDS70)",2]
[null,39,"0602.031300","00.3104","Модуль IGBT","IGBT Modual (GD100HFL120C2S)",2]
[null,40,"0602.024400","00.3091","Конденсатор","Capacitor (SFC-1200VDC/0.47uf)",2]
[null,41,"0602.023000","00.3077","Резонансная плата","Resonance plate (10031115)",1]
[null,42,"0601.041200","00.3123","Многоштырьковый разъем","6 pins control wire socket (MIG500-6X)",1]
[null,43,"0601.041300","00.3124","Розетка АС 36В","AC 36V heater (MIG500-AC36)",1]
[null,44,"0602.022100","00.3068","Предохранитель","Fuse (F-5A)",1]
[null,45,"0602.022200","00.3069","Кабельный ввод","Cable locker (M24)",1]
[null,46,"0602.031000","00.3101","Выключатель","Power switch (D50-50A)",1]
[null,47,"0601.041400","00.3125","Потенциометр","Burnback potentiometer (RV28P-B474)",1]
[null,48,"0601.051100","00.3142","Катушка индуктивная (входная)","Input inductance (MIG500-L4)",1]
[null,49,"0602.023700","00.3084","Плата управления","Driver board (1004291)",1]
[null,50,"0601.041600","00.3127","Трансформатор силовой","Power transformer (T11)",1]
[null,51,"0601.051200","00.3143","Трансформатор основной","Main transformer (MIG500-L5)",1]
[null,52,"0601.051300","00.3144","Фильтр обратной связи","Feedback signal shielding ring (MIG500-L6)",1]
[null,53,"0601.051400","00.3145","Плата контрольная","Control board (11072113-500)",1]
[null,54,"0601.042000","00.3131","Трансформатор силовой","Power transformer (T10)",1]
[null,55,"0601.051500","00.3146","Катушка индуктивеая","PI ring (MIG500-L7)",1]
[null,56,"0601.051600","00.3147","Кожух верхняя часть","Top side cover (MIG500-7)",1]
[null,57,"0602.032100","00.3112","Кольцо подъемное","Hanger ring (Φ35×M12)",2]
[null,58,"0601.051700","00.3148","Боковой упор для баллона","Gas cylinder trolley (MIG500-8)",2]
[null,59,"0602.022400","00.3071","Диод","Diode (1006188)",3]
[null,null,"0606.001800",null,"Горелка TIG с вентелем (Dх50) ",null,1]

{"sheet":"Блок MIG","index":1,"n_rows":47,"n_cols":8,"rows_kept":47,"flags":["formulas_cached_only"]}
[]
[null,"РАСКЛАДКА  ПОДАЮЩИЙ МЕХАНИЗМ АИС 500ПТ"]
{"$rows_empty":24}
[null,"Поз.","Код ELITECH","Артикул","Наименование","Описание (англ.)","Спецификация","Комплектация"]
[null,1,"0601.060000","00.3802","Корпус подающего механизма","Wire feeder body","SB-10-K-XT1",1]
[null,2,"0601.060100","00.3803","Стойки резиновые","Rubber foot 25×35","25×35",4]
[null,3,"0601.060200","00.3155","Разъем Dх50","Fasten connector DF 50-70","DF 50-70",1]
[null,4,"0601.060300","00.3805","Разъем 6-ти штырьковый","6pins control cable connector(Female)","6XZ",1]
[null,5,"0601.060400","00.3806","Держатель горелки","Torch holder","QJ",1]
[null,6,"0601.060500","00.3807","Крышка корпуса правая","Right side cover","YWK",1]
[null,7,"0601.060600","00.3808","Клапан газовый","Gas valve","DC24V",1]
[null,8,"0601.060700","00.3809","Рукоятка","Handle","TS",1]
[null,9,"0601.060800","00.3810","Кожух катушки","Plastic spool cover","FB-320",1]
[null,10,"0601.060900","00.3811","Панель контрольная","Control box","TJ-S01",1]
[null,11,"0601.061000","00.3821","Накладка панели","Scale panel","KD-01",1]
[null,12,"0601.061100","00.3813","Потенциометр","Voltage adjustment potentiometer","Rv24YN20SB502",1]
[null,13,"0601.061200","00.3813","Потенциометр","Current adjustment potentiometer","Rv24YN20SB502",1]
[null,14,"0601.061300","00.3815","Ручка потенциометра","Knob","A03",2]
[null,15,"0601.061400","00.3816","Кнопка протяжки проволоки","Inching","IPB-201",1]
[null,16,"0601.061500","00.3817","Крышка корпуса левая","Left side cover","ZWK",1]
[null,17,"0601.061600","00.3818","Разъем для горелки","Torch Euro connector",null,1]
[null,18,"0601.061700","00.3819","Механизм подачи в сборе","Motor assembly ","ZK76ZY-01",1]
[null,19,"0601.061800","00.3820","Электродвигатель","Motor","ZK76ZY02AV",1]
[null,20,"0601.060010","нет","Кабель межблочный 10м соединительный"]

{"sheet":"Подающий механизм","index":2,"n_rows":69,"n_cols":10,"rows_kept":69,"merged":[[1,1,1,7],[2,1,39,7]],"flags":["formulas_cached_only"]}
[]
[null,"РАСКЛАДКА  ПОДАЮЩИЙ МЕХАНИЗМ АИС 500ПТ"]
{"$rows_empty":28}
[{"$nulls":9},"4A"]
{"$rows_empty":9}
[null,"Поз.","Код ELITECH","Артикул","Наименование","Описание (англ.)","Спецификация","Комплектация"]
[null,1,"0601.061900","00.3822","Электродвигатель","Motor   ZK-60/76ZY01",null,1]
[null,2,"0601.062000","00.3823","Винт","Tighting screw",null,2]
[null,3,"0601.062100","00.3824","Приемник проволоки","Inlet guide nozzle",null,1]
[null,4,"0601.062200","00.3825","Корпус механизма подачи","Dual drive bracket",null,1]
[null,"4А","0601.062210","00.2848","Корпус механизма подачи в сборе с валами и прижимными роликами ","Wire feeder assembly",null,1]
[null,5,"0601.062300","00.3826","Вал ролика","Dualdrive feed roller shaft",null,2]
[null,6,"0601.062400",null,"Подшипник шестерни","Wire feed gear bearing",null,2]
[null,7,"0601.062500","00.3828","Штифт","Cylindrical pin",null,2]
[null,8,"0601.062600","00.3829","Шестерня","Dual drive gear",null,4]
[null,"8.1","0601.062601","00.3827","Шестерня в сборе с подшипником","Feeding gear with bearing",null,"1"]
[null,9,"0601.062700","00.3830","Шестерня главного привода","Wire feeder bearing",null,1]
[null,10,"0601.062800","00.3831","Втулка","Fixed gear gasket",null,2]
[null,11,"0601.062900","00.3832","Шайба  ","Feed roller",null,1]
[null,12,"0601.063000","00.3833","Ролик","Double drive wire feed",null,2]
[null,"12.1","0601.063001","00.4477","Ролик в сборе с втулкой",null,null,"1"]
[null,13,"0601.063100","00.3834","Шайба ролика","roller washer",null,2]
[null,14,"0601.063200","00.3835","Винт ролика","Knurled screw",null,2]
[null,15,"0601.063300","00.3836","Вал прижимного ролика","Pressure arm roller shaft",null,2]
[null,16,"0601.063400","00.3837","Ось суппорта","Dual drive pressure arm axial",null,2]
[null,17,"0601.063500","00.3838","Шайба пружинная","Spring washer",null,4]
[null,18,"0601.063600","00.3839","Суппорт прижимного ролика","Dual drive pressure arm ",null,2]
[null,19,"0601.063700","00.3840","Пружина торсионная","Pressure arm torsion spring",null,2]
[null,20,"0601.063800","00.3841","Коннектор выходной","Copper nut",null,1]
[null,21,"0601.063900","00.3842","Болт фиксатора фасонный","Pressure arm handle bolt",null,2]
[null,22,"0601.064000","00.3843","Втулка фиксатора","Pressure handle screw cover",null,2]
[null,23,"0601.064100","00.3844","Пружина фиксатора","Handle spring",null,2]
[null,24,"0601.064200","00.3845","Ручка фиксатора","Pressure handle knob",null,2]
[null,25,"0601.064300","00.3846","Канал средний","Middle guide in nozzle",null,1]

{"sheet":"Рисунки","index":3,"n_rows":43,"n_cols":1,"rows_kept":43,"merged":[[0,0,0,9],[19,0,19,9],[42,0,42,9]],"flags":["formulas_cached_only"]}
["0601.063001 Ролик в сборе с втулкой"]
{"$rows_empty":18}
["0601.062601 Шестерня в сборе с подшипником"]
{"$rows_empty":22}
["0601.061900 Motor ZK-60/76ZY01"]