{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":42,"n_cols":3,"rows_kept":42,"merged":[[1,0,1,2]],"flags":["formulas_cached_only"]}
["Product Code: 101532100"]
["Spare parts card"]
["N°","Product Code","Description"]
[1,7105292,"Base portacondensatore - Capacitor box base"]
[2,7102236,"Condensatore - Capacitor"]
[3,7105295,"Coperchio portacondensatore - Cover capacitor box"]
[4,360341,"Vite - Screw"]
[5,290241,"Vite - Screw"]
[6,290241,"Vite - Screw"]
[7,7002011,"Fermacavo - Cable locker"]
[8,7201060,"Cavo - Cable"]
[9,7103831,"Passacavo - Cable holder"]
[10,7201069,"Interruttore - Switch"]
[11,360341,"Vite - Screw"]
[12,3000319,"Morsettiera - Terminal box"]
[13,7105674,"Tirante - Screw"]
[14,7102174,"Copriventola - Fan cover"]
[15,7101796,"Ventola - Fan"]
[16,7101797,"Scudo - Shield"]
[17,1000250,"Anello compensazione - Spring washer"]
[18,7103147,"Statore - Stator"]
[19,1440100,"Cuscinetto - Ball bearing"]
[20,7105167,"Rotore - Rotor"]
[21,1440100,"Cuscinetto - Ball bearing"]
[22,7105512,"Corpo pompa inox - Stainless steel pump body"]
[23,7105810,"Tappo - Cap"]
[24,160812,"Vite - Screw"]
[25,1310517,"Anello OR - O-ring"]
[26,7105507,"Ugello venturi - Venturi nozzle"]
[27,7104970,"Diffusore - Diffuser disk"]
[28,1311487,"Anello OR - O-ring"]
[29,7105509,"Girante - Impeller"]
[30,3090479,"Tenuta meccanica - Mechanical seal"]
[31,3090809,"Tenuta meccanica - Mechanical seal"]
[32,1311537,"Anello OR - O-ring"]
[33,7107400,"Flangia portatenuta - Flange"]
[34,7103833,"Anello paragoccia - Packing"]
[35,7107404,"Supporto - Support"]
[36,7105844,"Maniglia - Handle"]
[37,290311,"Vite - Screw"]
[38,640052,"Dado - Nut"]
[39,7105845,"Maniglia - Handle"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}