{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["ТП3ЕР"],"not_rendered":{"images":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"ТП3ЕР","index":0,"n_rows":53,"n_cols":7,"rows_kept":53,"merged":[[0,0,30,6],[31,1,31,2],[31,3,31,5]],"flags":["formulas_cached_only"]}
{"$rows_empty":31}
["№","Артикул",null,"Описание",null,null,"Кол."]
[1,"1401.090000","GJJ0179 ","Накладка амортизирующая верхняя","Top silicone piece","上密封条",1]
["1А","1401.090001",null,"Термонагреватель в сборе ТП3ЕР"]
[2,"1401.090010","WWS12023","Кронштейн термонагревателя","PTC fixed frame","PTC固定框 ",2]
[3,"1401.090020",null,"Термостат KSD 302 25A 55 градусов","Self-reseting thermal cut-out",null,1]
[4,"1401.090030","GCY09008","Пластина крепления электродвигателя","Moto fixed plate","电机固定片",1]
["4А","1401.090031",null,"Электродвигатель с крыльчаткой в сборе ТП3ЕР"]
[5,"1401.090040","GCY09030  ","Кронштейн электродвигателя","Fan duct"," 风道固定框",1]
[6,"1401.090050","F0112-1 ","Электродвигатель YJ58-30 38 Ватт","Moto","电机",1]
[7,"1401.090060","WWS12025","Крыльчатка","Fan blade","风叶",1]
[8,"1401.090070",null,"Корпус верхняя часть","Shell",null,1]
[9,"1401.090080",null,"Рукоятка","Handle",null,1]
[10,"1401.090090",null,"Выключатель 15 Ампер 6 контактов","Switch",null,1]
[11,"1401.090100",null,"Ручка","Knob",null,1]
[12,"1401.090110 1401.066100 1401.001100 1401.055200",null,"Термостат регулируемый","Thermostat",null,1]
[13,"1401.090120","GJJ0179-1","Накладка амортизирующая нижняя","Bottom silicone piece","下密封条",1]
[14,"1401.090130",null,"Пластина крепления кронштейна электродвигателя","Duct fixed plate",null,1]
[15,"1401.090140",null,"Ножки","Feet",null,4]
[16,"1401.090150",null,"Корпус нижняя часть","Bottom",null,1]
[17,"1401.090160",null,"Фиксатор шнура питания","Cord buckle",null,1]
[18,"1401.090170",null,"Шнур питания","Power cord",null,1]
[19,"1401.090180","FR0303-1","Термонагреватель 3000 Ватт",null,"PTC发热体 ",1]